# Codelist Catalog

This report describes the ISO TC211 codelist catalogs, the codelists they contain, and the values and definitions of the codes.

Please contact Ted Habermann if you have questions or suggestions.

## Catalog

Name: Codelists from the Metadata for Reference System (mrs) Namespace
Scope: Codelists from the Metadata for Reference System (mrs) Namespace
Field of application: ISO TC211 Metadata Standards
Version: 0.1
Date: 2017-09-10
Number of CodeLists: 1
Number of items: 28

## Codelists

## MD_ReferenceSystemTypeCode :

Description: defines type of reference system used
CodeSpace: http://standards.iso.org/iso/19115/-3/mrs/1.0
Number of items: 28

Entry | Definition
--- | ---
compoundEngineeringParametric | compound statio-parametric coordinate reference system containing an engineering coordinate reference system and a parametric reference system. e.g. [local] x, y, pressure
compoundEngineeringParametricTemporal | compound statio-parametric-temporal coordinate reference system containing an engineering, a parametric, and a temporal coordinate reference system. e.g. [local] x, y, pressure, time
compoundEngineeringTemporal | compound spatio-temporal coordinate reference system containing an engineering and a temporal coordinate reference system. e.g. [local] x, y, time
compoundEngineeringVertical | compound spatial reference system containing a horizontal engineering coordinate reference system and a vertical coordinate reference system. e.g. [local] x, y, height
compoundEngineeringVerticalTemporal | compound spatio-temporal coordinate reference system containing an engineering, a vertical, and a temporal coordinate reference system. e.g. [local] x, y, height, time
compoundGeodeticParametric | compound statio-parametric coordinate reference system containing a 2 dimensional geographic horizontal coordinate reference system and a parametric reference system. e.g. latitude, longitude, pressure
compoundGeodeticParametricTemporal | compound statio-parametric-temporal coordinate reference system containing a 2 dimensional geographic horizontal, a parametric and a temporal coordinate reference system. e.g. latitude, longitude, pressure, time
compoundGeographic2DTemporal | compound spatio-temporal coordinate reference system containing a 2 dimensional geographic horizontal coordinate reference system and a temporal reference system. e.g. latitude, longitude, time
compoundGeographic2DVertical | compound coordinate reference system in which one constituent coordinate reference system is a horizontal geodetic coordinate reference system and one is a vertical coordinate reference system. e.g. latitude, longitude, [gravity-related] height or depth
compoundGeographicVerticalTemporal | compound spatio-temporal coordinate reference system containing a 2 dimensional geographic horizontal, a vertical, and a temporal coordinate reference system. e.g. latitude, longitude, height, time
compoundGeographic3DTemporal | compound spatio-temporal coordinate reference system containing a 3 dimensional geographic and a temporal coordinate reference system. e.g. latitude, longitude, ellipsoidal height, time
compoundProjected2DParametric | compound statio-parametric coordinate reference system containing a projected horizontal coordinate reference system and a parametric reference system. e.g. easting, northing, density
compoundProjected2DParametricTemporal | compound statio-parametric-temporal coordinate reference system containing a projected horizontal, a parametric, and a temporal coordinate reference system. e.g. easting, northing, density, time
compoundProjectedTemporal | compound spatio-temporal coordinate reference system containing a projected horizontal and a temporal coordinate reference system. e.g. easting, northing, time
compoundProjectedVertical | compound spatial reference system containing a horizontal projected coordinate reference system and a vertical coordinate reference system. e.g. easting, northing, [gravity-related] height or depth
compoundProjectedVerticalTemporal | compound spatio-temporal coordinate reference system containing a projected horizontal, a vertical, and a temporal coordinate reference system. e.g. easting, northing, height, time
engineering | coordinate reference system based on an engineering datum (datum describing the relationship of a coordinate system to a local reference). e.g. [local] x,y
engineeringDesign | engineering coordinate reference system in which the base representation of a moving object is specified. e.g. [local] x,y
engineeringImage | coordinate reference system based on an image datum (engineering datum which defines the relationship of a coordinate system to an image). e.g. row, column
geodeticGeocentric | geodetic CRS having a Cartesian 3D coordinate system. e.g. [geocentric] X,Y,Z
geodeticGeographic2D | geodetic CRS having an ellipsoidal 2D coordinate system. e.g. latitude, longitude
geodeticGeographic3D | geodetic CRS having an ellipsoidal 3D coordinate system. e.g. latitude, longitude, ellipsoidal height
geographicIdentifier | spatial reference in the form of a label or code that identifies a location. e.g. post code
linear | set of Linear Referencing Methods and the policies, records and procedures for implementing them. reference system that identifies a location by reference to a segment of a linear geographic feature and distance along that segment from a given point. e.g. x km along road
parametric | coordinate reference system based on a parametric datum (datum describing the relationship of a parametric coordinate system to an object). e.g. pressure
projected | coordinate reference system derived from a two-dimensional geodetic coordinate reference system by applying a map projection. e.g. easting, northing
temporal | reference system against which time is measured. e.g. time
vertical | one-dimensional coordinate reference system based on a vertical datum (datum describing the relation of gravity-related heights or depths to the Earth). e.g. [gravity-related] height or depth

top

Stylesheet: CT_CodelistHTML.xsl Version: 2017-09-10